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	Product characteristics 

	
(The text in red can be removed depending on your choice) 

	

	Installation:
This product is installed on a closed structure (e.g. a skylight), with or without mounting feet. 
Installation is possible with the box at the top or bottom, both indoors and outdoors. 
When mounting directly onto the window, the deflection of the bottom bar must be taken into account. 
If the Topfix® Large is installed over several glazed sections, the use of mounting feet is strongly recommended to avoid contact between the bottom bar and the window profile. 
The inclination angle can vary between 0° and 90°. The fabric type is selected according to the inclination angle.

Head box:

	Dimensions: 195 mm high x 150 mm deep. 

	Closed by a removable profile that rotates in the head box profile and can be dismantled. 

	Profiles are made of extruded aluminium. 

	The side brackets of the head box, which carry the roller mechanism and are fitted with pins, connect the box to the side guiding channels. 

	

	Roller tube:

	Made of galvanised steel. 

	Equipped with patented conical roller tube plugs to compensate for the thicker ends of the zip. 

	They also contain a tape reel for winding the tape. 

	The roller tube can be removed through the front of the box; viewed from this position, the left or right position is determined. 

	

	Fabric:

	All fabrics consist of one piece, except when the height is greater than the width of the fabric roll. 

	The fabrics are manufactured horizontally. 

	The vertical edges are fitted with a symmetrical zip, keeping the fabric windproof in the side guiding channel. 

	The zip is high-frequency welded, always on the least visible side. 


	● Polyester (semi-transparent):

	    Fire classification M1 (NFP 92503), B-s2,d0 (Euroclass EN 13501-1)

	    Weight: ± 380–420 g/m², thickness: 0.43–0.45 mm


	● Blackout polyester fabric:

	    Fire classification M2 (NFP 92503), B-s2,d0 (Euroclass EN 13501-1)

	    Weight: 650 g/m², thickness: 0.60 mm

Polyester fabric may show folds or waves.


	● PVC-free acryl fabric (semi-transparent & opaque):
     Fire classification M1 (NFP 92-503), B-s2,d0 (Euroclass EN 13501-1)
     Weight ± 450 g/m², thickness 0.55 mm




	Dimensions:

	Minimum width: 1200 mm. 

	Maximum width: 5000 mm and maximum projection: 6000 mm in one section. 

	Can be linked. Required spacing: 1 mm per 1000 mm width. 

	

	Side guiding channels:

	Made of 2 extruded aluminium profiles. 

	Dimensions: W 60 mm x D 75 mm side guide, 2-part. 

	Attachment to the head box is achieved by means of pins on the side brackets, which slide into the hollow chambers of the side guiding channel. 

	Each side guiding channel contains an HPVC zip guide with a co-extruded wear-resistant top layer (Smooth technology). 

	The HPVC zip guide is fitted with rubber profiles on each side to compensate for wind gusts. 

	The symmetrical zip welded to the fabric slides into this zip guide, thereby holding the fabric. 

	With correct installation, sufficient tolerance is provided between the fabric, aluminium side guiding channels and the HPVC zip guide to ensure smooth guidance. 

	

	Bottom bar:

	Made of 2 extruded aluminium profiles. 

	Dimensions of bottom bar: H 100 mm x D 62 mm. 

	

	Smooth-technologie

	Provides guidance for the bottom bar and fabric. 

	Thanks to the patented Smooth technology, the zip moves smoothly through the zip guide. 

	This intelligent zip guide is provided with a patented wear-resistant layer: 

	- guarantees optimal fabric tension 

	- eliminates the need for annual maintenance using a lubricant

	

	Tensioning system

	This revolutionary system pre-tensions the tape by means of a spring inside the roller tube. This spring is preloaded and maintains tension throughout the entire service life of the product. The tensioning system is unique in combination with our technology. This guarantees a windproof screen in every position. The tape running through the entire system is one continuous tape, ensuring that the system continues to operate safely in the event of tape damage or loss of tension, without damaging other system components (such as the fabric) or endangering bystanders. 

	

	Colour:

	All visible aluminium profiles (headbox, side guiding channels and bottom bar) can be powder-coated in the RAL colour (60–80 µm) matching the exterior joinery. 

	The side brackets are made of cast aluminium and painted in the same colour as the profiles.

	
Control:

	Electric: by means of a 230 VAC tubular motor, without emergency manual operation. 

	The connection is included in the sun protection package. 

	Supplied with a cable featuring a UV-resistant sheath. 

	Power supply and all wiring are included in the electrical package.

	


	Warranty:

	10-year warranty on all paintwork of the aluminium profiles. 

	5-year warranty on all defects that may occur under normal household use and regular maintenance. 

	5-year gloss warranty (paint finish). 

	5-year warranty on the electronic control system. 

	5-year warranty on the fabric collection.

	

	Wind class:

	Guaranteed up to 120 km/h in closed position when H (height of mounting feet) = 75 mm (EN 13561:2004+A1:2008, wind class 3 compliant). 
Guaranteed up to 80 km/h in closed position when H (height of mounting feet) = 150 mm (EN 13561:2004+A1:2008, wind class 3 compliant). 


	Standards and certificates:

	This product is manufactured according to, complies with and/or has been tested in accordance with the following standard: EN 13561. 



