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Aero Skye®
INTEGRATED PATIO COVER WITH ROTATABLE AND RETRACTABLE ALUMINIUM LOUVRES
Manufacturer
RENSON Outdoor nv, Polydore Rensonstraat 8, 9770 Kruisem – Belgium
Tel. +32(0)56 30 30 00, info@renson.be, www.renson-outdoor.com

(You can omit the text highlighted in red according to your choice)
Description
Aero Skye® is a horizontal patio cover integrated into an existing structure and equipped with a system of aluminium extruded, rotatable and retractable louvres.
Dimensions	
Span:	Min. 1800 mm
	Max. 4500 mm
Pivot:	Min. 3250 mm
	Max. 6200 mm

Free passage height: 	Dependent on the supporting structure

For your information:
The span side corresponds to the span of the blades.
The pivot side is the side on which the blades rotate (pivot)

System implementation
Frame:
· Aluminium‑extruded profiles, powder‑coated in a colour of your choice 
· Connections on the same side are finished in a single plane, without protruding cover caps or visible screws 
· Height: 260 mm 
· Height with louvres in vertical position: 260 mm + 95 mm 
· Depth of span‑frame profile: 150 mm 
· Depth of pivot‑frame profile: 330 mm 
· Inclination: 0°







Blades:
· Sun protection blades made of extruded aluminium
· Double-walled for handling a heavy snow load
· 135° rotatable (electronically controlled) 
· Slope: 3 cm over the full louvre length for optimal water drainage 
· Underside completely flat 
· Sides fitted with an L‑profile to prevent backflowing water, welded and coated in the same colour as the louvres 
· A triple-folded edge along the louvre length prevents residual water from dripping onto the terrace and furniture when the roof opens 
· Secured on the pivot sides using stainless‑steel shafts with integrated locking for a stable construction

Motorisation:
· 4 in-line 24 V DC motors with planetary transmission
· How it works
· Rotation: Worm and worm gear
· Retraction/opening: Synchronised spindles with a trolley and chain system
Even and guaranteed parallel sliding
· Placement: 
· The motors are invisibly integrated into the pivot profile

Water drainage:
· Downwards: One or more drainage openings of Ø50 mm are provided in the corner pieces or in the gutter. Each opening has a drainage trap that serves as a leaf catcher and forms the connection to a drain pipe (Ø50 mm) to be connected.
· Sidewards: A sideways-facing drainage pot in the corner pieces for drainage. It has a Ø50 mm to which a drain pipe (Ø50 mm) can be connected.

Assembly:
All fixings (e.g. screws) are invisibly made of stainless steel.

Colour:
All visible aluminum profiles are powder coated in textured paint, RAL color of your choice (60–80 microns).

Power supply and wiring:
Electrical cables are fully integrated, invisibly, into the terrace covering








Technical data:
Maximum weight of snow load:
Meets the static calculations according to DIN-EN regulations (Eurocode)
The load-bearing capacity depends on the dimensions and strength of the supporting structure.
With a maximum span of 4500mm, closed louvres have a load-bearing capacity of at least 520N/m².
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Maximum wind speed when controlling the blades:
120 km per hour (with closed blades)
160 km/h (with stacked blades)
Wind resistant up to:
50 km per hour (with closed blades)
Water drainage and precipitation rate:
The terrace covering can handle precipitation rate that corresponds to a rain shower with an intensity of 150 l/m2.h, which a maximum duration of 2 minutes. This type of rainfall occurs on average every 10 years. (Belgian rainfall statistics: NBN B 52-011) 

Warranty
· 10-year product warranty on the structure, subject to registration (all defects that may occur during normal household use and regular maintenance) (standard 5 years)
· 10-year warranty on the paint finish, color, and gloss of the aluminum profiles, subject to registration (standard 5 years)
· 5‑year warranty on Somfy and Renson motors. 
· 5‑year warranty on Somfy controls and sensors. 
· 5‑year warranty on Lineo Luce, Lineo Fix and Protecto
· 2‑year warranty on electrical components (heating, speakers, lighting, etc.)
· 2‑year warranty on the rain sensor




Options
Up/Down LED lighting:
Integrated LED lighting along the full length of the inner side of the frame equipped with direct and/or indirect lighting
· Up
· Warm white light, 120 LEDs/M | +/- 2800 K | 550-680 lumens/m
· Pure white light, 120 LEDs/M | +/- 5000 K | 550-680 lumens/m
· RGB 60 LEDs/m | 550-700 lumens/m

· Down
· Warm white light, 120 LEDs/M | +/- 2800 K | 550-680 lumens/m
· Pure white light, 120 LEDs/M | +/- 5000 K | 550-680 lumens/m

Beam heat & sound 
Beam:
· The patio cover can be equipped with a Beam module. This is an aluminium housing that can be fitted with heating elements (Heat) and speakers (Sound). 
· Can be mounted on the inside of the frame profiles on the span side. 
· The module can be continuously adjusted with a 30° pivoting range.

Heat:
· Heating element via radiant heat integrated in the Beam module.
· Heating element finished with flat black ceramic glass plate
· Power: 2400 W/Heat, Current = 12A/Heat, IP65
· RTS or IO control (same handheld transmitter as the louvres)
Sound:
· 4 Ohms Marine Speakers IP65 , 2 speakers integrated in the Beam module
· 120W Peak Power , Frequency Response: 90Hz - 22kHz 
· Cover plate in black anodised aluminium 
· To be connected to an amplifier / radio via the supplied audio cables or with integrated amplifier for autonomous operation and control via smartphone or tablet (incl. bluetooth)
· Dimensions W x H: 180 x 180 mm

Rain sensor kit: 
· Rain sensor, fixing materials and accessories
· Closes the blades automatically when there is rain
· It is mounted on a slight incline and has a tiny heating power element for better sensor drying

Wind, snow, frost:
· Adjustable via the app. Weather data is retrieved via the internet.

Norms
This product is made to conform to, satisfies and/or has been tested according to the norm: EN 13561
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