[image: ]Specifications
Aero® CANVAS
INTEGRATED CANOPY WITH FIXED ROOF
Manufacturer
RENSON Outdoor nv, Polydore Rensonstraat 8, 9770 Kruisem – Belgium
Tel. +32(0)56 30 30 00, info@renson.be, www.renson-outdoor.com

(You can omit the text highlighted in red according to your choice)
Description
Aero® Canvas is a horizontal aluminium canopy featuring an upper roof made of profiled steel sheeting and an aesthetic ceiling made of tightly tensioned fiberglass fabric, which is integrated into an existing structure. 

Dimensions
Span (longitudinal direction of the louvres):	min. 1200 mm – max. 4500 mm
	expandable with an intermediate beam up to max. span 6000 mm
Pivot (lateral direction of the louvres):	min. 2615 mm – max. 6055 mm
	

For your information:
The span side corresponds to the width of the steel sheets.
The pivot side is the side along which the different steel sheets are placed next to each other.

System implementation
Frame:
· A sturdy surrounding frame made of extruded aluminium profiles 
· Connection of adjacent frame profiles without corner caps
· Each frame profile is equipped with mounting brackets to fix the tensioned ceiling and the upper roof
· Height: 230 mm 
· Pitch/Slope: 0°


Upper roof:
· Profiled aluminium steel sheet, equipped on the underside with an anti‑condensation layer to prevent condensation droplets from falling onto the tensioned ceiling below
· The upper roof is fixed to the top frame via the mounting brackets





Ceiling:
· The fixed roof is finished on the underside with a horizontal fiberglass fabric, tensioned tightly using fabric‑tensioning profiles
· The fabric is attached all around using zippers, which secure it into a fabric‑tensioning profile and to the mounting brackets on the top frame
· The fabric‑tensioning profiles can be pulled closer to the frame, thereby tensioning the ceiling fabric and giving it a clean, taut appearance


Water drainage:
· The upper roof (steel sheet) is installed with a 20 mm slope. Water drains through a perforated profile on the side of the upper roof into the gutter, which is integrated into the profiles of the top frame and runs around the entire canopy. 
· Downwards: One or more drainage openings of Ø50 mm are provided in the corner pieces or in the gutter. Each opening has a drainage trap that serves as a leaf catcher and forms the connection to a drain pipe (Ø50 mm) to be connected.
· Sidewards: A sideways-facing drain pot runs from the inside of the frame to the outside of the frame. It has a Ø50 mm drain pipe to which a drain pipe (Ø50 mm) can be connected.

Assembly:
All fixings (e.g. screws) are invisibly made of stainless steel.

Colour:
All visible aluminum profiles are powder coated in textured paint, RAL color of your choice (60–80 microns).

Power supply and wiring:
Electrical cables are fully integrated, invisibly, into the terrace covering















Technical data:
Maximum weight of snow load:
[image: ]

Wind resistant up to:
120 km per hour 
	
Water drainage and precipitation rate:
The terrace covering can handle precipitation rate that corresponds to a rain shower with an intensity of 120 l/m2.h, which a maximum duration of 2 minutes. This type of rainfall occurs on average every 10 years. (Belgian rainfall statistics: NBN B 52-011) 

Warranty
· 10-year product warranty on the structure, subject to registration (all defects that may occur during normal household use and regular maintenance) (standard 5 years)
· 10-year warranty on the paint finish, color, and gloss of the aluminum profiles, subject to registration (standard 5 years)
· 5‑year warranty on Somfy and Renson motors. 
· 5‑year warranty on Somfy controls and sensors. 
· 5‑year warranty on Lineo Luce, Lineo Fix and Protecto
· 2‑year warranty on electrical components (heating, speakers, lighting, etc.)
· 2‑year warranty on the rain sensor




Options
Up/Down LED lighting:
Integrated LED lighting along the full length of the inner side of the frame equipped with direct and/or indirect lighting
· Up
· Warm white light, 120 LEDs/M | +/- 2800 K | 550-680 lumens/m
· Pure white light, 120 LEDs/M | +/- 5000 K | 550-680 lumens/m
· RGB 60 LEDs/m | 550-700 lumens/m

· Down
· Warm white light, 120 LEDs/M | +/- 2800 K | 550-680 lumens/m
· Pure white light, 120 LEDs/M | +/- 5000 K | 550-680 lumens/m

Norms
This product is made to conform to, satisfies and/or has been tested according to the norm: EN 13561
image1.png
. (mm)

Pivot

(mm) 1800 2000 2200 2400 2600 2800 3000 3200 3400 3600 3300 4000 4200 4400 4500
2615 133 1207 1097 1005 810 647 525 431 358 300 254 217 185 161 150
2830 1135 1022 928 B0 78 647 525 431 358 300 258 217 185 161 150
3045 973 875 795 728 671 622 525 431 358 300 254 217 185 161 150
3260 843 758 685 630 581 538 502 431 358 300 254 217 185 161 150
3475 737 662 601 S0 S07 470 438 410 355 300 254 217 185 161 150
3690 649 583 529 484 446 414 38 361 339 300 258 217 185 161 150
35 576 517 469 429 3% 367 342 320 300 283 254 217 185 161 150
4120 s 4@ 419 383 353 327 05 285 268 252 238 217 18 161 150
4335 461 414 376 344 316 293 273 255 240 226 214 202 18 161 150
4550 415 374 339 310 285 266 246 230 216 203 192 182 173 161 150
4765 37 33 307 281 258 239 223 208 195 184 174 165 156 149 145
4980 343 308 279 255 235 217 202 189 177 167 155 149 1e2 135 132
5195 306 274 249 227 209 193 18 168 157 148 140 132 126 120 117
5410 268 240 218 19 18 169 157 147 137 19 12 U5 100 104 102
5625 2% 211 191 175 160 148 138 19 120 113 107 101 9% 91 89
580 209 187 169 154 141 131 11 113 106 99 94 8 8 80 78
6055 185 166 150 136 125 116 107 100 93 8 8 78 74 70 68




image2.jpeg
22 RENSON'
reating healthy space




