,Width##LENGTH##MILLIMETERS,Wholesaler Art. No.##OTHER##,Wholesaler##OTHER##,Watermarked By##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,Vertical Right##OTHER##,Vertical Left##OTHER##,Flux Plus##OTHER##,Flux Go##OTHER##,Drain Fixture Units##OTHER##,EHA Y Offset##LENGTH##MILLIMETERS,Drain Wall Mounted Right Safe##OTHER##,Drain Wall Mounted Left Safe##OTHER##,Drain Diameter##LENGTH##MILLIMETERS,Drain Ceiling Mounted Right Safe##OTHER##,Drain Ceiling Mounted Right##OTHER##,Drain Ceiling Mounted Left Safe##OTHER##,Drain Ceiling Mounted Left##OTHER##,Connection Offset##LENGTH##MILLIMETERS,Horizontal Body##OTHER##,ETA Y Offset##LENGTH##MILLIMETERS,ETA X Offset##LENGTH##MILLIMETERS,EHA Connection##OTHER##,ODA Connection##OTHER##,ETA Connection##OTHER##,SUP Connection##OTHER##,Unit Weight (kg)##OTHER##,URL##OTHER##,Top Clearance##LENGTH##MILLIMETERS,Supply Air Flow 2##HVAC_AIR_FLOW##LITERS_PER_SECOND,Supply Air Flow 1##HVAC_AIR_FLOW##LITERS_PER_SECOND,Stabu Code##OTHER##,Service Space##OTHER##,Right Clearance##LENGTH##MILLIMETERS,Revit Version##OTHER##,Product Line##OTHER##,Power##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Phase##OTHER##,Model##OTHER##,Manufacturer URL##OTHER##,Manufacturer Art. No.##OTHER##,Manufacturer##OTHER##,MEPcontent Class##OTHER##,Length##LENGTH##MILLIMETERS,Left Clearance##LENGTH##MILLIMETERS,Internal Art. No.##OTHER##,IFCExportType##OTHER##,IFCExportAs##OTHER##,Horizontal Right##OTHER##,Horizontal Left##OTHER##,Hertz##ELECTRICAL_FREQUENCY##HERTZ,Height##LENGTH##MILLIMETERS,GTIN##OTHER##,GLN##OTHER##,Function Code##OTHER##,Front Clearance##LENGTH##MILLIMETERS,Family Version##OTHER##,Exhaust Air Flow 1##HVAC_AIR_FLOW##LITERS_PER_SECOND,Exhaust Air Flow 2##HVAC_AIR_FLOW##LITERS_PER_SECOND,ETIM Article Class##OTHER##,EMCS Version##OTHER##,Duct Diameter##LENGTH##MILLIMETERS,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Dark Black##OTHER##,Custom##OTHER##,Copyright##OTHER##,Content Supplier URL##OTHER##,CB-NL Class##OTHER##,Brown##OTHER##,Black##OTHER##,Base Family Version##OTHER##,Back Clearance##LENGTH##MILLIMETERS,Article Type##OTHER##,Article Description##OTHER##,Airflow Rate (m3/h)##OTHER##
FLUX GO Flat 225 Vertical Mounted Left,745,,,,230,0,1,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,340,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 225 Flat Vertical Mounted Left,https://renson.net/nl-be,76015068,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320588,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 225 Flat Vertical Mounted Left,"Central, demand-driven ventilation unit with heat recovery",225
FLUX GO Flat 225 Vertical Mounted Right,745,,,,230,1,0,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,760,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 225 Flat Vertical Mounted Right,https://renson.net/nl-be,76015068,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320588,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 225 Flat Vertical Mounted Right,"Central, demand-driven ventilation unit with heat recovery",225
FLUX GO Flat 275 Vertical Mounted Left,745,,,,230,0,1,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,340,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 275 Flat Vertical Mounted Left,https://renson.net/nl-be,76015069,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320595,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 275 Flat Vertical Mounted Left,"Central, demand-driven ventilation unit with heat recovery",275
FLUX GO Flat 275 Vertical Mounted Right,745,,,,230,1,0,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,760,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 275 Flat Vertical Mounted Right,https://renson.net/nl-be,76015069,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320595,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 275 Flat Vertical Mounted Right,"Central, demand-driven ventilation unit with heat recovery",275
FLUX GO Flat 370 Vertical Mounted Left,745,,,,230,0,1,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,340,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 370 Flat Vertical Mounted Left,https://renson.net/nl-be,76015070,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320601,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 370 Flat Vertical Mounted Left,"Central, demand-driven ventilation unit with heat recovery",370
FLUX GO Flat 370 Vertical Mounted Right,745,,,,230,1,0,0,1,0,102.5,0,0,32,0,0,0,0,182.746,0,997.5,760,0,0,0,0,25,,360,0,0,,0,360,2020,Renson Flux GO,0,1,FLUX GO 370 Flat Vertical Mounted Right,https://renson.net/nl-be,76015070,Renson,EXHAUST_UNIT,1188,360,,NOTDEFINED,IfcAirTerminalBox,0,0,50,300,5413470320601,5413470000008,,360,23.08,0,0,EC010004,5,160,"Central, demand-driven ventilation unit with heat recovery",0,Color RGB 030-030-030,0,© Trimble Europe BV,www.MEPcontent.com,,Color RGB 138-110-075,Color RGB 043-043-044,24.04,360,FLUX GO 370 Flat Vertical Mounted Right,"Central, demand-driven ventilation unit with heat recovery",370
