;REN_I Glass thickness_min##LENGTH##MILLIMETERS;REN_I Glass thickness_max##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_20Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_2Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_10Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_V Glass thickness##LENGTH##MILLIMETERS;RSen_C_code_article##OTHER##;RSen_C_description##OTHER##;REN_I Equivalent area (mm2/m)##OTHER##;REN_I Free area (mm2/m)##OTHER##
window ventilation_renson_TC60_h 75_20;20;20;Installation above glass/traverse;44,28;198;62,64;140,04;20;TC60_20;renson_window ventilation_TC60_20;15652;12314
window ventilation_renson_TC60_h 75_24;24;24;Installation above glass/traverse;44,28;198;62,64;140,04;24;TC60_24;renson_window ventilation_TC60_24;15652;12314
window ventilation_renson_TC60_h 75_28;28;28;Installation above glass/traverse;44,28;198;62,64;140,04;28;TC60_28;renson_window ventilation_TC60_28;15652;12314
