;RSen_C_model##OTHER##;RSen_C_type_comments##OTHER##;RSen_C_description##OTHER##;RSen_C_type##OTHER##;REN_I Shape##OTHER##;REN_V Supply air##OTHER##;REN_V Air exhaust##OTHER##;ZZZ_Recess depth_Length##LENGTH##MILLIMETERS;REN_I Flange_height##LENGTH##MILLIMETERS;RSen_C_depth##LENGTH##MILLIMETERS;REN_I Flange_thickness min##LENGTH##MILLIMETERS;REN_I Flange_thickness max##LENGTH##MILLIMETERS;REN_I Flange_thickness##LENGTH##MILLIMETERS;REN_I Depth_min##LENGTH##MILLIMETERS;REN_I Depth_max##LENGTH##MILLIMETERS;REN_I Width_min##LENGTH##MILLIMETERS;REN_I Height_min##LENGTH##MILLIMETERS;REN_I Diameter_min##LENGTH##MILLIMETERS;REN_I Width_max##LENGTH##MILLIMETERS;REN_I Height_max##LENGTH##MILLIMETERS;REN_I Size_maximum##OTHER##;REN_I Diameter_max##LENGTH##MILLIMETERS;REN_I Blade_shape##OTHER##;REN_I Blade_type##OTHER##;REN_I Blade_pitch##LENGTH##MILLIMETERS;REN_I Control##OTHER##;REN_I Visual free area##OTHER##;REN_I Zichtbaar vrije opp.##OTHER##;REN_I K factor_intake##OTHER##;REN_I K factor_discharge##OTHER##;REN_I Ce coefficient_intake##OTHER##;REN_I Cd coefficient_discharge##OTHER##;REN_I Puncture proof##OTHER##;REN_I IP##OTHER##;REN_I Sound reduction_Rw##OTHER##;REN_I Sound reduction_Dw##OTHER##;REN_I Burglarproof_WK class##OTHER##;REN_I Fire resistance##OTHER##;REN_I U-value##OTHER##;REN_I Without flange_info##OTHER##;REN_I Without flange##OTHER##;REN_I Drainage profile##OTHER##;REN_I Water channel##OTHER##;REN_I Removable insect mesh##OTHER##;REN_I G4 filter##OTHER##;REN_I Backframe##OTHER##;REN_I Material##OTHER##;REN_I Glazed in##OTHER##;ZZZ_Profile top_offset_Length##LENGTH##MILLIMETERS;ZZZ_Profile bottom_minimum height_Length##LENGTH##MILLIMETERS;ZZZ_Louvre_insertion point_Length##LENGTH##MILLIMETERS;ZZZ_Flange_offset_Length##LENGTH##MILLIMETERS;REN_I Backframe_min wall thickness##LENGTH##MILLIMETERS;REN_I Backframe_max wall thickness##LENGTH##MILLIMETERS;ZZZ_Flange_FamilyType_Air Terminals##OTHER##;ZZZ_Louvre_FamilyType_Air Terminals##OTHER##;RSen_C_code_article##OTHER##
414thf/24 - glazed-in louvre - rectangular - exhaust air flow_renson_414;414THF;glazed-in louvre;renson_414thf - thermally broken;thermally broken;rectangular;0;1;24;20;47,5;24;32;24;0;0;130;130;0;2500;2500;see price list;0;Z;L.033.01;33,3;-;0;0;20,47;19,58;0,221;0,226;1;IP2XD;-;-;-;-;1,1;no;0;0;0;0;0;0;aluminiumAlMgSi0.5;1;69;23;0;26;19;71,5;GEO_flange_renson : standard;GEO_louvre_renson : standard;414THF/24
414thf/28 - glazed-in louvre - rectangular - exhaust air flow_renson_414;414THF;glazed-in louvre;renson_414thf - thermally broken;thermally broken;rectangular;0;1;28;20;51,5;24;32;28;0;0;130;130;0;2500;2500;see price list;0;Z;L.033.01;33,3;-;0;0;20,47;19,58;0,221;0,226;1;IP2XD;-;-;-;-;1,1;no;0;0;0;0;0;0;aluminiumAlMgSi0.5;1;69;23;0;26;19;71,5;GEO_flange_renson : standard;GEO_louvre_renson : standard;414THF/28
414thf/32 - glazed-in louvre - rectangular - exhaust air flow_renson_414;414THF;glazed-in louvre;renson_414thf - thermally broken;thermally broken;rectangular;0;1;32;20;55,5;24;32;32;0;0;130;130;0;2500;2500;see price list;0;Z;L.033.01;33,3;-;0;0;20,47;19,58;0,221;0,226;1;IP2XD;-;-;-;-;1,1;no;0;0;0;0;0;0;aluminiumAlMgSi0.5;1;69;23;0;26;19;71,5;GEO_flange_renson : standard;GEO_louvre_renson : standard;414THF/32
