	RSen_C_model##OTHER##	RSen_C_type_comments##OTHER##	RSen_C_description##OTHER##	RSen_C_type##OTHER##	REN_I Shape##OTHER##	REN_V Supply air##OTHER##	REN_V Air exhaust##OTHER##	ZZZ_Recess depth_Length##LENGTH##MILLIMETERS	REN_I Flange_height##LENGTH##MILLIMETERS	RSen_C_depth##LENGTH##MILLIMETERS	REN_I Flange_thickness min##LENGTH##MILLIMETERS	REN_I Flange_thickness max##LENGTH##MILLIMETERS	REN_I Flange_thickness##LENGTH##MILLIMETERS	REN_I Depth_min##LENGTH##MILLIMETERS	REN_I Depth_max##LENGTH##MILLIMETERS	REN_I Width_min##LENGTH##MILLIMETERS	REN_I Height_min##LENGTH##MILLIMETERS	REN_I Diameter_min##LENGTH##MILLIMETERS	REN_I Width_max##LENGTH##MILLIMETERS	REN_I Height_max##LENGTH##MILLIMETERS	REN_I Size_maximum##OTHER##	REN_I Diameter_max##LENGTH##MILLIMETERS	REN_I Blade_shape##OTHER##	REN_I Blade_type##OTHER##	REN_I Blade_pitch##LENGTH##MILLIMETERS	REN_I Control##OTHER##	REN_I Visual free area##OTHER##	REN_I Zichtbaar vrije opp.##OTHER##	REN_I K factor_intake##OTHER##	REN_I K factor_discharge##OTHER##	REN_I Ce coefficient_intake##OTHER##	REN_I Cd coefficient_discharge##OTHER##	REN_I Puncture proof##OTHER##	REN_I IP##OTHER##	REN_I Sound reduction_Rw##OTHER##	REN_I Sound reduction_Dw##OTHER##	REN_I Burglarproof_WK class##OTHER##	REN_I Fire resistance##OTHER##	REN_I U-value##OTHER##	REN_I Without flange_info##OTHER##	REN_I Without flange##OTHER##	REN_I Drainage profile##OTHER##	REN_I Water channel##OTHER##	REN_I Removable insect mesh##OTHER##	REN_I G4 filter##OTHER##	REN_I Backframe##OTHER##	REN_I Material##OTHER##	REN_I Glazed in##OTHER##	ZZZ_Profile top_offset_Length##LENGTH##MILLIMETERS	ZZZ_Profile bottom_minimum height_Length##LENGTH##MILLIMETERS	ZZZ_Louvre_insertion point_Length##LENGTH##MILLIMETERS	ZZZ_Flange_offset_Length##LENGTH##MILLIMETERS	REN_I Backframe_min wall thickness##LENGTH##MILLIMETERS	REN_I Backframe_max wall thickness##LENGTH##MILLIMETERS	ZZZ_Flange_FamilyType_Air Terminals##OTHER##	ZZZ_Louvre_FamilyType_Air Terminals##OTHER##	RSen_C_code_article##OTHER##
414thf/24 - glazed-in louvre - rectangular - supply air flow_renson_414	414THF	glazed-in louvre	renson_414thf - thermally broken	thermally broken	rectangular	1	0	24	20	47,5	24	32	24	0	0	130	130	0	2500	2500	see price list	0	Z	L.033.01	33,3	-	0,59	0,50	20,47	19,58	0,221	0,226	1	IP2XD	-	-	-	-	1,1	no	0	0	0	0	0	0	aluminiumAlMgSi0.5	1	69	23	0	26	19	71,5	GEO_flange_renson : standard	GEO_louvre_renson : standard	414THF/24
414thf/28 - glazed-in louvre - rectangular - supply air flow_renson_414	414THF	glazed-in louvre	renson_414thf - thermally broken	thermally broken	rectangular	1	0	28	20	51,5	24	32	28	0	0	130	130	0	2500	2500	see price list	0	Z	L.033.01	33,3	-	0,59	0,50	20,47	19,58	0,221	0,226	1	IP2XD	-	-	-	-	1,1	no	0	0	0	0	0	0	aluminiumAlMgSi0.5	1	69	23	0	26	19	71,5	GEO_flange_renson : standard	GEO_louvre_renson : standard	414THF/28
414thf/32 - glazed-in louvre - rectangular - supply air flow_renson_414	414THF	glazed-in louvre	renson_414thf - thermally broken	thermally broken	rectangular	1	0	32	20	55,5	24	32	32	0	0	130	130	0	2500	2500	see price list	0	Z	L.033.01	33,3	-	0,59	0,50	20,47	19,58	0,221	0,226	1	IP2XD	-	-	-	-	1,1	no	0	0	0	0	0	0	aluminiumAlMgSi0.5	1	69	23	0	26	19	71,5	GEO_flange_renson : standard	GEO_louvre_renson : standard	414THF/32
