;REN_I Airflow opening##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_20Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_2Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_10Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_I Sound reduction Dn,e,w (C,Ctr)_in open position##OTHER##;RSen_C_code_article##OTHER##;RSen_C_description##OTHER##;REN_I Equivalent area (mm2/m)##OTHER##;REN_I Free area (mm2/m)##OTHER##
window ventilation_renson_Sonovent® Compact_h 95_10;10;Installation above glass/traverse;43,56;64,08;59,04;62,28;36 (0,-1) dB;SONOVENT® Compact 10;renson_window ventilation_SONOVENT® Compact 10;15334;9500
window ventilation_renson_Sonovent® Compact_h 95_13;13;Installation above glass/traverse;54,72;67,32;67,68;67,68;35 (0,-1) dB;SONOVENT® Compact 13;renson_window ventilation_SONOVENT® Compact 13;19278;12500
window ventilation_renson_Sonovent® Compact_h 95_15-20;15;Installation above glass/traverse;69,84;70,92;71,64;66,96;33 (0,-1) dB;SONOVENT® Compact 15;renson_window ventilation_SONOVENT® Compact 15;24687;15000
