;RSen_C_model##OTHER##;RSen_C_type_comments##OTHER##;RSen_C_description##OTHER##;RSen_C_type##OTHER##;REN_I Shape##OTHER##;REN_V Supply air##OTHER##;REN_V Air exhaust##OTHER##;ZZZ_Recess depth_Length##LENGTH##MILLIMETERS;REN_I Flange_height##LENGTH##MILLIMETERS;RSen_C_depth##LENGTH##MILLIMETERS;REN_I Flange_thickness min##LENGTH##MILLIMETERS;REN_I Flange_thickness max##LENGTH##MILLIMETERS;REN_I Flange_thickness##LENGTH##MILLIMETERS;REN_I Depth_min##LENGTH##MILLIMETERS;REN_I Depth_max##LENGTH##MILLIMETERS;REN_I Width_min##LENGTH##MILLIMETERS;REN_I Height_min##LENGTH##MILLIMETERS;REN_I Diameter_min##LENGTH##MILLIMETERS;REN_I Width_max##LENGTH##MILLIMETERS;REN_I Height_max##LENGTH##MILLIMETERS;REN_I Size_maximum##OTHER##;REN_I Diameter_max##LENGTH##MILLIMETERS;REN_I Blade_shape##OTHER##;REN_I Blade_type##OTHER##;REN_I Blade_pitch##LENGTH##MILLIMETERS;REN_I Control##OTHER##;REN_I Visual free area##OTHER##;REN_I Zichtbaar vrije opp.##OTHER##;REN_I K factor_intake##OTHER##;REN_I K factor_discharge##OTHER##;REN_I Ce coefficient_intake##OTHER##;REN_I Cd coefficient_discharge##OTHER##;REN_I Puncture proof##OTHER##;REN_I IP##OTHER##;REN_I Sound reduction_Rw##OTHER##;REN_I Sound reduction_Dw##OTHER##;REN_I Burglarproof_RC class##OTHER##;REN_I Fire resistance##OTHER##;REN_I U-value##OTHER##;REN_I Without flange_info##OTHER##;REN_I Without flange##OTHER##;REN_I Drainage profile##OTHER##;REN_I Water channel##OTHER##;REN_I Removable insect mesh##OTHER##;REN_I G4 filter##OTHER##;REN_I Backframe##OTHER##;REN_I Material##OTHER##;REN_I Glazed in##OTHER##;ZZZ_Profile top_offset_Length##LENGTH##MILLIMETERS;ZZZ_Profile bottom_minimum height_Length##LENGTH##MILLIMETERS;ZZZ_Louvre_insertion point_Length##LENGTH##MILLIMETERS;ZZZ_Flange_offset_Length##LENGTH##MILLIMETERS;ZZZ_Flange_FamilyType_Air Terminals##OTHER##;ZZZ_Louvre_FamilyType_Air Terminals##OTHER##;RSen_C_code_article##OTHER##
484/24 - glazed-in louvre - rectangular - supply air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;1;0;40;31;51;24;32;24;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/24
484/28 - glazed-in louvre - rectangular - supply air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;1;0;42;31;51;24;32;28;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/28
484/32 - glazed-in louvre - rectangular - supply air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;1;0;44;31;51;24;32;32;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/32
484/24 - glazed-in louvre - rectangular - exhaust air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;0;1;40;31;51;24;32;24;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/24
484/28 - glazed-in louvre - rectangular - exhaust air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;0;1;42;31;51;24;32;28;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/28
484/32 - glazed-in louvre - rectangular - exhaust air flow_renson_484;484;glazed-in louvre;renson_484 - heavy-duty series;heavy-duty;rectangular;0;1;44;31;51;24;32;32;0;0;220;220;0;4000;4000;see price list;0;Z;L.050HF;50;-;0,7;0,6;9,41;9,47;0,326;0,325;1;IP2XD;-;-;-;-;-;no;0;1;1;1;1;0;aluminiumAlMgSi0.5;1;104;50;1;42;GEO_flange_renson : standard;GEO_louvre_renson : standard;484/32
