**EASYFLEX Round duct Ø80mm**

**G0013131**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

Round ducts are usually used on vertical lengths up to the ventilation system. We recommend a 80mm diameter for spaces with an air flow rate of < 50 m3/h.

The length of the concrete duct (G0013133) is 25 cm.

PRODUCT CHARACTERISTICS

* Made of PVC RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

