**EASYFLEX flat oval duct**

**G0013126**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

The flat oval duct is made of PVC and has an outer diameter of 135 x 55 mm, and an equivalent inner diameter of 90 mm. The limited height of the Easyflex® air duct makes it easy to recess in screed, concrete or stud walls or false ceilings.

The air duct’s broad cross section allows high air flow rates at low velocities, which leads to quiet ventilation system operation.

PRODUCT CHARACTERISTICS

* Made of PVC RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

