**EASYFLEX Valve connection Ø125mm**

**G0013117**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

You can make seamless connections between RENSON® design extraction louvres or SQair valves and valve connectors in an Easyflex® air duct system. Valve connectors come in two diameters: Ø80mm in-line connectors for spaces with an extraction air flow rate ≤ 50 m3/h and Ø125mm for spaces with an extraction air flow rate ≥ 50 m3/h.

You can connect extraction grills directly to the valve transits, if they are built into a Gyproc wall. If the extraction louvre is fitted in a vaulted surface, you can use a connector that you can saw along its length. You can also use valve connectors as a connecting piece to join flat, oval ducts to round

ducts.

PRODUCT CHARACTERISTICS

* Made of polypropylene RAL 9002
* Anti-static and antibacterial
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

