**EASYFLEX Round duct Ø125mm**

**G0013130**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

Round ducts are usually used on vertical lengths up to the ventilation system. We recommend a 125mm diameter for spaces with an air flow rate of > 50 m3/h.

The 125 mm round duct is characterized by its very low pressure drop. High air flow rates are achievable at low air flow velocities.

The length of the concrete duct (G0013132) is 25 cm.

PRODUCT CHARACTERISTICS

* Made of PVC RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

