**EASYFLEX Y-piece**

**2x140x60mm > 140x60mm**

**G0013120**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

It is possible to connect one flat, oval channel to two flat, oval channels. In this way, two spaces can be reached with a single main channel.

For example, extraction from two rooms can be done on one valve. To do this, controllable grate bases must be installed to adjust the flow rates.

PRODUCT CHARACTERISTICS

* Made of PVC RAL 9002
* Anti-static and antibacterial
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

