**EASYFLEX double Valve connection Ø125mm**

**G0013118**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

You can make seamless connections between RENSON® design extraction louvres and valve connectors in an Easyflex® air duct system. Double valve connectors are used for spaces requiring high air flow rates.

You can connect extraction grills directly to the valve transits, if they are built into a Gyproc wall. If the extraction louvre is fitted in a vaulted structure, you use a connecting piece that can be sawn in its length.

You can also use a double valve connection as a connecting piece to join flat, oval ducts to round ducts.

PRODUCT CHARACTERISTICS

* Made of polypropylene RAL 9002
* Anti-static and antibacterial
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

