**easyflex Connector with integrated rubber gaskets, round Ø80mm**

**g0013121**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

description

The unique coupling system ensures an almost perfect airtightness. The connector is equipped with two integrated double rubber seals. Thanks to these seals, the Easyflex® air duct system qualifies for airtightness class D, meaning the system is three times less liable to leak than class C.

The coupling can be reinforced with PVC tape (66014115).

product characteristics

* Made of polypropylene
* Rubber sealing: TPE (ThermoPlastic Elastomer)
* Airtightness class D
* Smooth inner wall
* Low air flow resistance
* Easy to clean

APPLICATION

* The round connector Ø 80 mm can be used to couple:
* Round duct Ø 80 mm (G0013131)
* Concrete duct Ø 80 mm (G0013133)
* All accessories Ø 80 mm