**EASYFLEX Distribution box angled 160mm**

**G0013135**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

The distribution box is part of the Easyflex® range. This distribution box has an angled main connection of 160 mm and there are up to 6 ducts that can be connected to it.

By joining the distribution box to the supply and extract ducts of a ventilation system D, an easy installation is guaranteed. The Easyflex® ducts can directly be connected to the distribution box by means of the supplied Easyflex® fastening brackets (G0013137).

The limited height of the Easyflex® distribution box makes it easy to recess the box and its ducts in screed, concrete or stud walls or false ceilings.

The distribution box’s broad cross section and the tube connections allow high air flow rates at low velocities, which leads to quiet ventilation system operation.

PRODUCT CHARACTERISTICS

* Made of HDPE RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

