**EASYFLEX vertical bend 90°**

**G0013114**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

It is best to avoid using flexible ducts for sharp bends. It is better to use fixed bend accessories, such as a 90° vertical bend.

PRODUCT CHARACTERISTICS

* Made of polypropylene RAL 9002
* Anti-static and antibacterial
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

