**EASYFLEX Straight double adaptor**

**2 x 140 x 60 mm > Ø125mm**

**G0013141**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

A connection can be made from two flat, oval channels to a round duct using a straight adaptor piece Ø125mm for areas with an extraction flow > 50 m3/h. The extraction grids can be coupled directly to the straight adaptor if incorporated in a plasterboard wall.

The adaptors may also be used as a transition piece between the flat oval ducts and the round ducts.

PRODUCT CHARACTERISTICS

* Made of polypropylene RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

