**EASYFLEX Adaptor flat to round**

**140 x 60 mm > Ø125mm**

**G0013124**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

You can make a transition connection between the oval and round duct by using an in-line connector. You can use Ø 80 mm in-line connectors for spaces with an extraction air flow rate ≤ 50 m3/h and Ø125mm for spaces with an extraction air flow rate ≥ 50 m3/h. You can connect extraction grills directly to in-line connectors, if they are built into a Gyproc wall.

And you can use in-line connectors to join flat, oval ducts to round ducts.

PRODUCT CHARACTERISTICS

* Made of polypropylene RAL 9002
* Anti-static and antibacterial
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

