**EASYFLEX Distribution box 8 connections**

**G0013136**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

The distribution box is part of the Easyflex® range. This distribution box can provide supply using two Easyflex® ducts and can be connected to up to six ducts. In this way, the distribution box can be placed centrally, rather than coupled directly to the main duct. The two supply lines can be coupled using the double valve connection (G0013118) or the straight double adapter (G0013141).

By joining the distribution box to the supply and extract ducts of a ventilation system D, an easy installation is guaranteed. The Easyflex® ducts can directly be connected to the distribution box by means of the supplied Easyflex® fastening brackets (G0013137).

The limited height of the Easyflex® distribution box makes it easy to recess the box and its ducts in screed, concrete or stud walls or false ceilings.

The distribution box’s broad cross section and the tube connections allow high air flow rates at low velocities, which leads to quiet ventilation system operation.

PRODUCT CHARACTERISTICS

* Made of HDPE RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

