**EASYFLEX Flexible duct**

**G0013110**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

Easyflex® is a flexible polyethylene duct with an outer diameter of 140 x 64 mm and an equivalent inner diameter of 90 mm. The smooth inner wall of this double walled duct has an anti-static and antibacterial additive treatment to help prevent dust build-up and bacterial outbreaks. The limited height of the Easyflex® air duct makes it easy to recess in screed, concrete or stud walls or false ceilings.

The air duct’s broad cross section allows high air flow rates at low velocities, which leads to a quiet ventilation system operation.

PRODUCT CHARACTERISTICS

* Double walled
  + Ribbed outer sheath
  + Smooth inner sheath
* Made of polyethylene
  + Outer sheath: HDPE RAL 9002
  + Inner sheath: LDPE
* Antibacterial and anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

