**easyflex Inspection hatch**

**76050405**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

description

Each distribution box can be transformed into a distribution box with inspection hatch within a few minutes. The screws are included and make sure that the inspection hatch can be installed (opened and closed) in no time at all. It can be built in at the top as at the bottom and is therefore fit for use in screed, concrete, stud walls or false ceilings.

The durable inspection hatch of high quality, allows a permanent access to the Easyflex® air duct system for cleaning and/or inspecting its parts. The inspection date, the person responsible and all possible remarks can be indicated on the inspection label, so that maintenance can continuously and precisely be followed-up.

Thanks to the sealing foam there is perfect tightness of the air duct system, so that the air flow is optimized.

product characteristics

* Made of galvanized steel
* Sealing foam

APPLICATION

* The inspection hatch can be built-in in:
* Distribution box straight 160 mm (G0013140)
* Distribution box angled 160 mm (G0013135)
* Distribution box 8 connections (G0013136)