**easyflex Connector with integrated rubber gaskets, flat**

**g0013111**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

description

The unique coupling system ensures an almost perfect airtightness. The connector is equipped with two integrated double rubber seals.

Thanks to these seals, the Easyflex® air duct system qualifies for airtightness class D, meaning the system is three times less liable to leak than class C.

product characteristics

* Made of polypropylene
* Rubber sealing: TPE (ThermoPlastic Elastomer)
* Airtightness class D
* Smooth inner wall
* Low air flow resistance
* Easy to clean

APPLICATION

* The flat connector can be used to couple:
* The Easyflex® flexible duct (G0013110)
* The Easyflex® flat oval duct (G0013126)
* Coupling of all Easyflex® accessories
* The coupling can be reinforced with:
* Quick fastener (G0013112)
* Metal fastening bracket (G0013137)