;REN_V Glass thickness##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_20Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_2Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_10Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_I THL100##OTHER##;REN_V Transom##OTHER##;RSen_C_code_article##OTHER##;RSen_C_model##OTHER##;RSen_C_description##OTHER##;REN_I Equivalent area (mm2/m)##OTHER##;REN_I Free area (mm2/m)##OTHER##
window ventilation_renson_THL100V_h 144_15;15;Installation above glass/traverse;36;163,8;51,12;115,56;0;0;THL100V_15;THL100V;renson_window ventilation_THL100V_15;12770;27950
window ventilation_renson_THL100V_h 144_20;20;Installation above glass/traverse;36;163,8;51,12;115,56;0;0;THL100V_20;THL100V;renson_window ventilation_THL100V_20;12770;27950
window ventilation_renson_THL100V_h 144_24;24;Installation above glass/traverse;36;163,8;51,12;115,56;0;0;THL100V_24;THL100V;renson_window ventilation_THL100V_24;12770;27950
window ventilation_renson_THL100V_h 144_28;28;Installation above glass/traverse;36;163,8;51,12;115,56;0;0;THL100V_28;THL100V;renson_window ventilation_THL100V_28;12770;27950
