;RSen_C_height##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;RSen_M_flow_rate_Q_at_2Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_10Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_C_code_article##OTHER##;RSen_C_description##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_20Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_I Equivalent area (mm2/m)##OTHER##;REN_I Free area (mm2/m)##OTHER##
Window Ventilation_Renson_T100;100;Installation above glass;70,2;157,68;T100;renson_window ventilation_T100;48,96;222,84;17326;16368
Window Ventilation_Renson_T130;130;Installation above glass;99,72;223,56;T130;renson_window ventilation_T130;69,48;316,44;24589;16368
Window Ventilation_Renson_T150;150;Installation above glass;114,84;257,4;T150;renson_window ventilation_T150;79,2;363,6;27992;16368
