;Flow_Rate_Qnom_l/s/m##HVAC_AIR_FLOW##LITERS_PER_SECOND;Flow_Rate_Qnom_m³/h/m##OTHER##;Installation##OTHER##;Depth_Ventilation##LENGTH##MILLIMETERS;Height_Ventilation##LENGTH##MILLIMETERS;Max._Length##LENGTH##MILLIMETERS;Watertightness_In_Open_Position, up to##HVAC_PRESSURE##PASCALS;U-value (W/m²K)##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN;Sound_Reduction_Dn,e,w(C,Ctr)_in open position##OTHER##;Sound_Reduction_Dn,e,w(C,Ctr)_in closed position##OTHER##;Voltage_of_Device (internal)##OTHER##;Voltage##OTHER##;Burglar_Proof##OTHER##;Condensation_Free##OTHER##;Ventil1##OTHER##;Ventil2##OTHER##;T2x1##OTHER##;T2x2##OTHER##;T2x3##OTHER##;T2x4##OTHER##;T2x5##OTHER##;T2x6##OTHER##
Endura Twist - 2x1;3.33;12;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;1;0;1;0;0;0;0;0
Endura Twist - 2x2;6.67;24;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;0;1;0;1;0;0;0;0
Endura Twist - 2x3;10;36;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;0;1;0;0;1;0;0;0
Endura Twist - 2x4;13.33;48;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;0;1;0;0;0;1;0;0
Endura Twist - 2x5;16.67;60;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;0;1;0;0;0;0;1;0
Endura Twist - 2x6;20;72;On top of the window profile;345;110;6000;150;1;40 (0,-3) dB;50,6 (-3,-7) dB;15 V DC;230 V / 50 Hz;Class WK2;Yes;0;1;0;0;0;0;0;1
