;REN_V Glass thickness##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_20Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_2Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;RSen_M_flow_rate_Q_at_10Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_I THL100##OTHER##;REN_V Transom##OTHER##;RSen_C_code_article##OTHER##;RSen_C_model##OTHER##;RSen_C_description##OTHER##;REN_I Equivalent area (mm2/m)##OTHER##;REN_I Free area (mm2/m)##OTHER##
window ventilation_renson_THL100_h 144_15;15;Installation above glass/traverse;47,52;212,04;67,32;149,76;1;0;THL100_15;THL100;renson_window ventilation_THL100_15;16759;16200
window ventilation_renson_THL100_h 144_20;20;Installation above glass/traverse;47,52;212,04;67,32;149,76;1;0;THL100_20;THL100;renson_window ventilation_THL100_20;16759;16200
window ventilation_renson_THL100_h 144_24;24;Installation above glass/traverse;47,52;212,04;67,32;149,76;1;0;THL100_24;THL100;renson_window ventilation_THL100_24;16759;16200
window ventilation_renson_THL100_h 144_28;28;Installation above glass/traverse;47,52;212,04;67,32;149,76;1;0;THL100_28;THL100;renson_window ventilation_THL100_28;16759;16200
