;Thickness_Window_Frame_MIN##LENGTH##MILLIMETERS;Thickness_Window_Frame_MAX##LENGTH##MILLIMETERS;Thickness_Window_Frame##OTHER##;Depth_Ventilation##LENGTH##MILLIMETERS;Max._Length##LENGTH##MILLIMETERS;Installation##OTHER##;Watertightness_In_Open_Position, up to##HVAC_PRESSURE##PASCALS;Watertightness_In_Closed_Position, up to##HVAC_PRESSURE##PASCALS;U-value (W/m²K)##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN;Sound_Reduction_Dn,e,w(C,Ctr)_in open position##OTHER##;Sound_Reduction_Dn,e,w(C,Ctr)_in closed position##OTHER##;Self-regulating_Valve##OTHER##;Length_Total##LENGTH##MILLIMETERS;Height_Void##LENGTH##MILLIMETERS;Flow_Rate_Q_at_10Pa_m³/h/m##OTHER##;Flow_Rate_Q_at_10Pa_l/s/m##HVAC_AIR_FLOW##LITERS_PER_SECOND;Equivalent_Area##OTHER##;Depth_Void_Front##LENGTH##MILLIMETERS;Depth_Void_Back##LENGTH##MILLIMETERS;Depth_Facade##LENGTH##MILLIMETERS;Control_Options_Internal_Flap##OTHER##;Burglar_Proof##OTHER##;Aluminium_Profile##OTHER##;Air_Leakage_at 50 Pa##OTHER##;X2##LENGTH##MILLIMETERS;108##OTHER##;138##OTHER##;168##OTHER##;198##OTHER##;228##OTHER##;258##OTHER##;288##OTHER##;Design_Cap_HR##OTHER##
Invisivent Air UT - 50-82;50;82;50-82mm;108;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;1;0;0;0;0;0;0;0
Invisivent Air UT - 83-112;83;112;83-112mm;108;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;1;0;0;0;0;0;0;0
Invisivent Air UT - 113-142;113;142;113-142mm;138;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;1;0;0;0;0;0;0
Invisivent Air UT - 143-172;143;172;143-172mm;168;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;1;0;0;0;0;0
Invisivent Air UT - 173-202;173;202;173-202mm;198;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;1;0;0;0;0
Invisivent Air UT - 203-232;203;232;203-232mm;228;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;1;0;0;0
Invisivent Air UT - 233-262;233;262;233-262mm;258;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;0;1;0;0
Invisivent Air UT - 263-292;263;292;263-292mm;288;6000;On top of the window profile;250;900;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;0;0;1;0
Invisivent Air HR UT - 50-82;50;82;50-82mm;108;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;1;0;0;0;0;0;0;1
Invisivent Air HR UT - 83-112;83;112;83-112mm;108;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;1;0;0;0;0;0;0;1
Invisivent Air HR UT - 113-142;103;142;113-142mm;138;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;1;0;0;0;0;0;1
Invisivent Air HR UT - 143-172;143;172;143-172mm;168;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;1;0;0;0;0;1
Invisivent Air HR UT - 173-202;173;202;173-202mm;198;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;1;0;0;0;1
Invisivent Air HR UT - 203-232;203;232;203-232mm;228;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;1;0;0;1
Invisivent Air HR UT - 233-262;233;262;233-262mm;258;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;0;1;0;1
Invisivent Air HR UT - 263-292;263;292;263-292mm;288;6000;On top of the window profile;250;1200;1.8;"34 (0;-1) dB";"51 (-1;-3) dB";Yes (I-Flux technology);1000;85.50;117.6 m³/h/m;32.70;12246 mm²/m;200;500;150;Motor, Manual, Cord, Rod;Class WK2;EL/EV1,RAL, Bicolor;<15% (in closed position);13;0;0;0;0;0;0;1;1
