;REN_I Thickness window frame_MIN##LENGTH##MILLIMETERS;REN_I Thickness window frame_MAX##LENGTH##MILLIMETERS;REN_I Installation##OTHER##;REN_V Window frame depth##LENGTH##MILLIMETERS;REN_I Sound reduction Dn,e,w (C,Ctr)_in open position##OTHER##;REN_I Sun protection_max height##LENGTH##MILLIMETERS;REN_I U-value##HVAC_COEFFICIENT_OF_HEAT_TRANSFER##WATTS_PER_SQUARE_METER_KELVIN;RSen_C_depth##LENGTH##MILLIMETERS;Type Comments##OTHER##;Description##OTHER##;RSen_C_code_article##OTHER##;RSen_M_flow_rate_Q_at_1Pa##HVAC_AIR_FLOW##CUBIC_METERS_PER_HOUR;REN_I Equivalent area (mm2/m)##OTHER##
Recessed - Acoustic and ventilation - Top of the window - Box 167x132(S) - Access internal - AK;50;94;Installation overframe;50;33 (0,-2) dB;3000;1,47;167;Window ventilation and sun protection;renson_window ventilation_fixvent mono ak evo small;Fixvent Mono AK EVO Small;46,08;18324
Recessed - Acoustic and ventilation - Top of the window - Box 197x132(M) - Access internal - AK;95;124;Installation overframe;95;35 (0,-3) dB;3000;0,98;197;Window ventilation and sun protection;renson_window ventilation_fixvent mono ak evo medium;Fixvent Mono AK EVO Medium;46,08;18324
Recessed - Acoustic and ventilation - Top of the window - Box 227x132(L) - Access internal - AK;125;154;Installation overframe;125;36 (-1,-4) dB;3000;0,8;227;Window ventilation and sun protection;renson_window ventilation_fixvent mono ak evo large;Fixvent Mono AK EVO Large;46,08;18324
Recessed - Acoustic and ventilation - Top of the window - Box 257x132(XL) - Access internal - AK;155;184;Installation overframe;155;37 (-1,-4) dB;3000;0,77;257;Window ventilation and sun protection;renson_window ventilation_fixvent mono ak evo X-large;Fixvent Mono AK EVO X-Large;46,08;18324
Recessed - Acoustic and ventilation - Top of the window - Box 287x132(XXL) - Access internal - AK;185;215;Installation overframe;185;40 (-1,-4) dB;3000;0,72;287;Window ventilation and sun protection;renson_window ventilation_fixvent mono ak evo XX-large;Fixvent Mono AK EVO XX-Large;46,08;18324
Recessed - Acoustic and ventilation - Top of the window - Box 167x132(S) - Access internal - UT;50;94;Installation overframe;50;33 (0,-2) dB;3000;1,47;167;Window ventilation and sun protection;renson_window ventilation_fixvent mono ut evo small;Fixvent Mono UT EVO Small;55,80;19724
Recessed - Acoustic and ventilation - Top of the window - Box 197x132(M) - Access internal - UT;95;124;Installation overframe;95;35 (0,-3) dB;3000;0,98;197;Window ventilation and sun protection;renson_window ventilation_fixvent mono ut evo medium;Fixvent Mono UT EVO Medium;55,80;19724
Recessed - Acoustic and ventilation - Top of the window - Box 227x132(L) - Access internal - UT;125;154;Installation overframe;125;36 (-1,-4) dB;3000;0,8;227;Window ventilation and sun protection;renson_window ventilation_fixvent mono ut evo large;Fixvent Mono UT EVO Large;55,80;19724
Recessed - Acoustic and ventilation - Top of the window - Box 257x132(XL) - Access internal - UT;155;184;Installation overframe;155;37 (-1,-4) dB;3000;0,77;257;Window ventilation and sun protection;renson_window ventilation_fixvent mono ut evo X-large;Fixvent Mono UT EVO X-Large;55,80;19724
Recessed - Acoustic and ventilation - Top of the window - Box 287x132(XXL) - Access internal - UT;185;215;Installation overframe;185;40 (-1,-4) dB;3000;0,72;287;Window ventilation and sun protection;renson_window ventilation_fixvent mono ut evo XX-large;Fixvent Mono UT EVO XX-Large;55,80;19724
