,XXL##OTHER##,XL##OTHER##,With_Fixvent_Filler_Profile##OTHER##,Uniclass 2015 Description##OTHER##,Uniclass 2015 Code##OTHER##,URL##OTHER##,Suitable for Utility Building##OTHER##,Suitable for Residential Building##OTHER##,S##OTHER##,Renson_Specification_Document##OTHER##,Renson_Product_Type##OTHER##,Renson_Product_Installation_Method##OTHER##,Renson_Product_Brochure##OTHER##,Renson_Minimum_Width##LENGTH##MILLIMETERS,Renson_Minimum_Height##LENGTH##MILLIMETERS,Renson_Maximum_Width##LENGTH##MILLIMETERS,Renson_Maximum_Height##LENGTH##MILLIMETERS,Renson_Maximum_Area##AREA##SQUARE_METERS,Renson_Materials_Fabric##OTHER##,Renson_Materials_Blind_Hardwear##OTHER##,Renson_Logo##OTHER##,Renson_Filler_Profile_lengte##LENGTH##MILLIMETERS,Renson_Box_Type##OTHER##,Renson_Blind_Area##AREA##SQUARE_METERS,OmniClass Description##OTHER##,OmniClass Code##OTHER##,Model##OTHER##,Manufacturer##OTHER##,M##OTHER##,L##OTHER##,Input_Total_Width##LENGTH##MILLIMETERS,Input_Total_Height##LENGTH##MILLIMETERS,Input_Fabric_Roller_Height##LENGTH##MILLIMETERS,Input_Fabric_Materials_Polyester##OTHER##,Input_Fabric_Materials_Fiberglass##OTHER##,Input_Fabric_Materials_Blackout##OTHER##,IfcExportType[Type]##OTHER##,IfcExportAs[Type]##OTHER##,Effective_Renson_Filler_profile_Lengte##LENGTH##MILLIMETERS,ETIM-7.0##OTHER##,Dimensions Optional Filler Profile (for thinner window profile)##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Compatible Window Thickness##OTHER##
"Recessed - Acoustic and ventilation - Top of the window - Box 167x132(S) - Access internal",0,0,0,External roller blinds,Pr_30_59_07_26,https://www.renson.eu/,FIXVENT MONO UT,FIXVENT MONO AK,1,https://www.renson.eu,FIXVENT MONO AK/UT (S),MS4,https://www.renson.eu,1000.000000000000,300.000000000000,2000.000000000000,2700.000000000000,5.400000000000,<By Category>,Aluminum,1,0.600000000000,Small,1.200000000000,Exterior Protection of Openings ,23-17 21 11,FIXVENT MONO AK (S),RENSON,0,0,1000.000000000000,1200.000000000000,500.000000000000,0,0,1,SHUTTER,IfcShadingDeviceType,-0.600000000000,EC003229,No filler profile,1219.200000000000,50-94 mm
"Recessed - Acoustic and ventilation - Top of the window - Box 197x132(M) - Access internal",0,0,1,External roller blinds,Pr_30_59_07_26,https://www.renson.eu/,FIXVENT MONO UT,FIXVENT MONO AK,0,https://www.renson.eu,FIXVENT MONO AK/UT (M),MS4,https://www.renson.eu,1000.000000000000,300.000000000000,2000.000000000000,2700.000000000000,5.400000000000,<By Category>,Aluminum,1,30.000000000000,Medium,1.200000000000,Exterior Protection of Openings ,23-17 21 11,FIXVENT MONO AK (M),RENSON,1,0,1000.000000000000,1200.000000000000,500.000000000000,0,0,1,SHUTTER,IfcShadingDeviceType,-30.000000000000,EC003229,30 mm,1219.200000000000,95-124 mm
"Recessed - Acoustic and ventilation - Top of the window - Box 227x132(L) - Access internal",0,0,1,External roller blinds,Pr_30_59_07_26,https://www.renson.eu/,FIXVENT MONO UT,FIXVENT MONO AK,0,https://www.renson.eu,FIXVENT MONO AK/UT (L),MS4,https://www.renson.eu,1000.000000000000,300.000000000000,2000.000000000000,2700.000000000000,5.400000000000,<By Category>,Aluminum,1,60.000000000000,Large,1.200000000000,Exterior Protection of Openings ,23-17 21 11,FIXVENT MONO AK (L),RENSON,0,1,1000.000000000000,1200.000000000000,500.000000000000,0,0,1,SHUTTER,IfcShadingDeviceType,-60.000000000000,EC003229,60 mm,1219.200000000000,125 -154 mm
"Recessed - Acoustic and ventilation - Top of the window - Box 257x132(XL) - Access internal",0,1,1,External roller blinds,Pr_30_59_07_26,https://www.renson.eu/,FIXVENT MONO UT,FIXVENT MONO AK,0,https://www.renson.eu,FIXVENT MONO AK/UT (XL),MS4,https://www.renson.eu,1000.000000000000,300.000000000000,2000.000000000000,2700.000000000000,5.400000000000,<By Category>,Aluminum,1,90.000000000000,X-Large,1.200000000000,Exterior Protection of Openings ,23-17 21 11,FIXVENT MONO AK (XL),RENSON,0,0,1000.000000000000,1200.000000000000,500.000000000000,0,0,1,SHUTTER,IfcShadingDeviceType,-90.000000000000,EC003229,90 mm,1219.200000000000,155 -184 mm
"Recessed - Acoustic and ventilation - Top of the window - Box 287x132(XXL) - Access internal",1,0,1,External roller blinds,Pr_30_59_07_26,https://www.renson.eu/,FIXVENT MONO UT,FIXVENT MONO AK,0,https://www.renson.eu,FIXVENT MONO AK/UT (XXL),MS4,https://www.renson.eu,1000.000000000000,300.000000000000,2000.000000000000,2700.000000000000,5.400000000000,<By Category>,Aluminum,1,120.000000000000,XX-Large,1.200000000000,Exterior Protection of Openings ,23-17 21 11,FIXVENT MONO AK (XXL),RENSON,0,0,1000.000000000000,1200.000000000000,500.000000000000,0,0,1,SHUTTER,IfcShadingDeviceType,-120.000000000000,EC003229,120 mm,1219.200000000000,185 -215 mm
