**EASYFLEX flexible connection piece**

**G0013139**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

The Easyflex® connection piece can be used to connect flat oval ducts (G0013126) and flexible ducts (G0013110). The connection piece consists of a 350 mm flexible air duct with a connection sleeve with rubber along both sides. It can also be used for horizontal and vertical curves of 90° at the most, but as well for other difficult obstacle points (for instance S-curves). The flexible connection piece has an outer diameter of 140 x 64 mm and an equivalent inner diameter of 90 mm.

The air duct’s broad cross section allows high air flow rates at low velocities, which leads to a quiet ventilation system operation.

The limited height of the Easyflex® connection piece makes it easy to recess in stud walls or false ceilings. It can also be poured in screed or concrete as long as strengthening or reinforcement is provided.

The smooth finished inner wall has an anti-static additive treatment to help prevent dust build-up and bacterial outbreaks.

PRODUCT CHARACTERISTICS

* Single walled
  + Ribbed out sheath
* Made of polyethylene
  + HDPE RAL 9002
* Anti-static
* Airtightness class D

(as long as tape is used)

* Smooth inner wall

pressure drop

