**EASYFLEX Cross piece pivot**

**G0013145**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – België

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

DESCRIPTION

The cross piece is a part of the Easyflex® range. This cross piece makes it possible to cross lines with a height of 65 mm.

The pivoting feature ensures you can determine the angle in which the lines cross each other for yourself. In this way, no extra distances and turns are required to meet a 90° angle. With the pivot cross piece, it is possible to bridge angles from 45° to 135°.

Bridging obstacles up to 3 cm in height is also possible with this piece. Support with ‘pur’ is recommended.

PRODUCT CHARACTERISTICS

* Made of HDPE RAL 9002
* Anti-static
* Airtightness class D
* Smooth inner wall
  + Low air flow resistance
  + Easy to clean

pressure drop

